**Testing with TuskSAR**

**Step 1 to Step 3:** Same as <https://wiki.humaxdigital.com/display/AIWT/Mobile+client+testing+for+G-AX27+Router>

(build frontend with: **npm run build:TurkSAT:intg**)

Except from:

After connect successfully, type login id (root) and password (humax@!0416) and type ***sh*** to change the prompt

**Step 4:** Show HSRGApp pid by:

>> ps aux | grep HS



Kill HSRGApp pid:

>> kill -9 <pid>

EX: In this case:

>> kill -9 4845

**Step 5:** Copy test.tar.gz file and decompression

Using command:

>> cd /mnt/apps/www\_root

>> rm –rf \*

>> tftp –gr test.tar.gz 192.168.1.x (PC IP)

Decompression (on Router)

>> tar zxvf test.tar.gz

**Step 6:** Restart HSRGAPP:

Using command:

>> HSRGApp -m 0 &

Wait a little bit for completing web server.